### current community

- chat
  Electrical Engineering
- Electrical Engineering Meta

### your communities

Sign up or log in to customize your list.

### more stack exchange communities

company blog
Stack Exchange Inbox Reputation and Badges
sign up log in tour help

- Tour Start here for a quick overview of the site
- Help Center Detailed answers to any questions you might have
- Meta Discuss the workings and policies of this site
- About Us Learn more about Stack Overflow the company
- Business Learn more about hiring developers or posting ads with us

Electrical Engineering
_
Electrical Engineering Stack Exchange is a question and answer site for electronics and electrical engineering professionals, students, and enthusiasts. Join them; it only takes a minute:
Sign up
Here's how it works:

1. Anybody can ask a question
2. Anybody can answer
3. The best answers are voted up and rise to the top

# Understanding purpose of components in a half bridge driver circuit

up vote 2 down vote favorite 1 | I'm currently trying to learn and understand about creating an H-Bridge using two half bridge drivers. The half bridge drivers I have are IR2184. I found a circuit diagram someone else has designed using the same driver ICs but I have some questions about it.

I've seen several similar circuits where resistors are placed in line with the gates of the mosfets - What are those resistors for?

Also on the circuit above the designer has placed some diodes parallel to those resistors. Is there a reason for doing that?

mosfet mosfet-driver full-bridge

| asked Nov 9 '14 at 14:16 m3z 122 6

add a comment |

## 4 Answers 4

active oldest votes

up vote 1 down vote accepted | You should always provide a gate resistor. At the very least it actually helps define the current that will flow in and out of the GATE during switching transients (to charge and discharge the gate capacitance). Without any gate resistor you could have very large (relatively speaking) peak currents flowing. Best-case... its an EMC concern, worst-case... you potentially burn out the gate of the FET.

You also run the risk of creating a Pierce Oscillator.

In this instance you can see a series gate resistance with a diode in parallel. This limits the current and thus the switching time for TURN-ON.

The diode then "shorts" the resistor out permitting a higher charge transfer for a TURN-OFF.

This is a cheap/simple means to mitigate shoot-through's of a H-bridge leg during PWM transitions as you now have fast TURN-OFF and slow TURN-ON

| answered Nov 9 '14 at 14:40 JonRB 7,538 2 11 25

add a comment |

up vote 2 down vote | The resistors in series with the MOSFET gates are damping resistors. They reduce the tendency of the circuit to oscillate or ring when switching. The diodes in parallel look like they are intended to speed up the discharge of the MOSFET's gate capacitance when the signal goes from HIGH to LOW. So, they help the MOSFETs switch off faster.

| answered Nov 9 '14 at 14:28 John Honniball 2,065 4 8

add a comment |

up vote 1 down vote | Because FET input has gate capacitance, and the driver usually has strong current source capacity. So, when with no resistor, the current spike may cause EMI problem, and other problems. So adding series resistor to slow-down the switching. But usually, we needs to shut down the FET faster, adding of the damping resistor will slow down the discharging of the gate capacitance too. With reverse paralleled diode, when the gate capacitor discharge, the current will flow in the diode, but not the damping resistor, this makes the shut down faster than turning on.

| answered Nov 9 '14 at 14:45 diverger 3,240 10 31

add a comment |

up vote 1 down vote | There's another important reason to the presence of the diode antiparalled to the gate resistor. In a bridge configuration, when a transitor goes on the switching, the voltage acroos the other transitor has a increased dV/dt. In a MOSFET, that's the case of your H-brigde, there's three intrinsic capacitances composing its bory, like in the image below (that shows other stray components of the Mosfet bory):

When the Vds voltage increases, all the three capacitances need to be charged, like in the schematic below:

simulate this circuit – Schematic created using CircuitLab

Where the red arrows are current flowing through the circuit (when Vds are increasing).

So, if this resistance of the discharge isn't low, the Cgs capacitange could had a peak of charge, creating a short-time short-circuit, named punch through.

More information at this app. note

http://www.irf.com/technical-info/appnotes/an-936.pdf

| answered Feb 25 '15 at 3:22 Luis Possatti 38 5

add a comment |

## Your Answer

draft saved
draft discarded

### Sign up or log in

Sign up using Google

Sign up using Facebook

Sign up using Email and Password

### Post as a guest

Name Email

discard

By posting your answer, you agree to the privacy policy and terms of service.

## Not the answer you're looking for? Browse other questions tagged mosfet mosfet-driver full-bridge or ask your own question.

question feed