Arduino

Reference Language | Libraries | Comparison | Changes

LiquidCrystal

## setCursor()

#### Description

Position the LCD cursor; that is, set the location at which subsequent text written to the LCD will be displayed.

#### Syntax

lcd.setCursor(col, row)

#### Parameters

lcd: a variable of type LiquidCrystal

col: the column at which to position the cursor (with 0 being the first column)

row: the row at which to position the cursor (with 0 being the first row) Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes