==================================

LT Slave USB Driver Manual

==================================

1. One full pack of driver should include£º
   MPC6535USB2.0 Driver.exe
   RWIniFile.dll
   LTSetupCfg.ini
   LTUSB.inf
   ezusb.sys

2. This driver is compatible with£º
   MPC6515/MPC6535/MPC6575/MPC6536/MPC6610

3. If "find new hardware" appears in computer screen at the first time, please click "cancel".

4. Run "MPC6535USB2.0 Driver.exe" and intall the driver.

5. After the driver installation, unplug and plug in again the USB-interface cable.

6. If "find new hardware" appears in computer screen, please let it set up aumatically.
======================
April 2010
Leetro Automation Co., Ltd
www.leetro.com
Tech@leetro.com
======================