


Merry Christmas fellow programmers.
	
Thanks for downloading TWODEER.DXF!
	
This DXF file is compatable with Autocad, Smartcam, Rhino, Bobcad,
CorelDraw, HiJaak Pro, and any other CAD CAM CNC program that will
accept a DXF formatted file (I do not know of any CNC program that will
not Import this file)
This file was drawn in Autocad, imported into Smartcam and later 
coded as a Komo Router program using a Fanuc control. 
	
TWODEER.DXF was written for a 4" X 8" Komo 508 Router.
The .DXF file can be scaled to fit any size CNC workspace. 
The original program was written to cut .500 thick plywood, the slotted
areas where the TWODEER components are assembled are set up to
be run with cutter comp. Depending on your material thickness and
tool width, the slot widths will possibly need to be adjusted and most
certainly need to be adjusted should the artwork be scaled to fit inside
a CNC with a smaller work envelope.
I have even scaled this DXF down and cut "baby deer" from 1/8" thick
aluminum plate. 
	
Origin of this file?  I did not create the original pattern of this DXF. 
I had a router customer approach me to see if I could write a CNC
program of TWODEER, the customer furnished me a "band sawed"
set of deer that he had been given in 1998.  I spent one hour with
a tape measure and a legal pad, the TWODXF deer were created later
that same 	evening.
	
Enjoy!  
	
Michael Gailey
http://www.microsystemsgeorgia.com/toc.htm
gailey@frontiernet.net
	
	












